(export (version D)
  (design
    (source C:\Users\Joris\Documents\kicad\sma2_plug_v2\sma2_plug_v2.sch)
    (date "2020-05-31 18:29:39")
    (tool "Eeschema (5.1.5)-3")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "SMA2 Plug v2")
        (company)
        (rev 2.1)
        (date 2020-05-31)
        (source sma2_plug_v2.sch)
        (comment (number 1) (value "Licensed under CERN-OHL-S v2 https://cern.ch/cern-ohl"))
        (comment (number 2) (value "Copyright 2020 Joris van Rantwijk"))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J3)
      (value Conn_02x06_Top_Bottom)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x06_Odd_Even) (description "Generic connector, double row, 02x06, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5F93EF))
    (comp (ref U2)
      (value 74LVC126)
      (footprint Package_SO:SOIC-14_3.9x8.7mm_P1.27mm)
      (datasheet http://www.ti.com/lit/gpn/sn74LS126)
      (libsource (lib 74xx) (part 74LS126) (description "Quad buffer 3-State outputs"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E603A4E))
    (comp (ref U1)
      (value 74LVC126)
      (footprint Package_SO:SOIC-14_3.9x8.7mm_P1.27mm)
      (datasheet http://www.ti.com/lit/gpn/sn74LS126)
      (libsource (lib 74xx) (part 74LS126) (description "Quad buffer 3-State outputs"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E6295DE))
    (comp (ref J1)
      (value Conn_Coaxial)
      (footprint Connector_Coaxial:SMA_Samtec_SMA-J-P-X-ST-EM1_EdgeMount)
      (datasheet " ~")
      (libsource (lib Connector) (part Conn_Coaxial) (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E629612))
    (comp (ref R3)
      (value 33)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E629618))
    (comp (ref R4)
      (value 33)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E629620))
    (comp (ref R5)
      (value 33)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E629626))
    (comp (ref R8)
      (value 50)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E629645))
    (comp (ref C3)
      (value 1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E65DDA0))
    (comp (ref C4)
      (value 100nF)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E65E58F))
    (comp (ref C1)
      (value 1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E69295B))
    (comp (ref C2)
      (value 100nF)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E692961))
    (comp (ref R9)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E615CAC))
    (comp (ref R10)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E638303))
    (comp (ref R1)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E696119))
    (comp (ref R2)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E69611F))
    (comp (ref J2)
      (value Conn_Coaxial)
      (footprint Connector_Coaxial:SMA_Samtec_SMA-J-P-X-ST-EM1_EdgeMount)
      (datasheet " ~")
      (libsource (lib Connector) (part Conn_Coaxial) (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E60806F))
    (comp (ref R7)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E7810C1))
    (comp (ref R13)
      (value 33)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E60A55C))
    (comp (ref R12)
      (value 33)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E60A204))
    (comp (ref R11)
      (value 33)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E6087B4))
    (comp (ref R14)
      (value 33)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EF7A2DB))
    (comp (ref R6)
      (value 33)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F0E1442))
    (comp (ref JP2)
      (value Jumper_3_Open)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Jumper) (part Jumper_3_Open) (description "Jumper, 3-pole, both open"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F1ABB3C))
    (comp (ref R15)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E73F947))
    (comp (ref R16)
      (value 50)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E76DD7C))
    (comp (ref JP1)
      (value Jumper_3_Open)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Jumper) (part Jumper_3_Open) (description "Jumper, 3-pole, both open"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F2BA64E)))
  (libparts
    (libpart (lib 74xx) (part 74LS126)
      (description "Quad buffer 3-State outputs")
      (docs http://www.ti.com/lit/gpn/sn74LS126)
      (footprints
        (fp DIP*W7.62mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS126))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name ~) (type 3state))
        (pin (num 4) (name ~) (type input))
        (pin (num 5) (name ~) (type input))
        (pin (num 6) (name ~) (type 3state))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name ~) (type 3state))
        (pin (num 9) (name ~) (type input))
        (pin (num 10) (name ~) (type input))
        (pin (num 11) (name ~) (type 3state))
        (pin (num 12) (name ~) (type input))
        (pin (num 13) (name ~) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib Connector) (part Conn_Coaxial)
      (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)")
      (docs " ~")
      (footprints
        (fp *BNC*)
        (fp *SMA*)
        (fp *SMB*)
        (fp *SMC*)
        (fp *Cinch*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_Coaxial))
      (pins
        (pin (num 1) (name In) (type passive))
        (pin (num 2) (name Ext) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x06_Odd_Even)
      (description "Generic connector, double row, 02x06, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x06_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Jumper) (part Jumper_3_Open)
      (description "Jumper, 3-pole, both open")
      (docs ~)
      (footprints
        (fp SolderJumper*Open*))
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_3_Open))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name C) (type input))
        (pin (num 3) (name B) (type passive)))))
  (libraries
    (library (logical 74xx)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/74xx.lib"))
    (library (logical Connector)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Connector.lib"))
    (library (logical Connector_Generic)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Connector_Generic.lib"))
    (library (logical Device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Device.lib"))
    (library (logical Jumper)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Jumper.lib")))
  (nets
    (net (code 1) (name GND)
      (node (ref R8) (pin 2))
      (node (ref R16) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref R9) (pin 2))
      (node (ref R10) (pin 2))
      (node (ref J3) (pin 4))
      (node (ref J3) (pin 3))
      (node (ref U1) (pin 7))
      (node (ref R15) (pin 1))
      (node (ref C2) (pin 2))
      (node (ref U2) (pin 7))
      (node (ref C4) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref J2) (pin 2))
      (node (ref R7) (pin 1))
      (node (ref R2) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref J1) (pin 2)))
    (net (code 2) (name "Net-(R12-Pad2)")
      (node (ref U2) (pin 6))
      (node (ref R12) (pin 2)))
    (net (code 3) (name "Net-(R11-Pad2)")
      (node (ref R11) (pin 2))
      (node (ref U2) (pin 3)))
    (net (code 4) (name "Net-(R13-Pad2)")
      (node (ref R13) (pin 2))
      (node (ref U2) (pin 8)))
    (net (code 5) (name +3V3)
      (node (ref U1) (pin 13))
      (node (ref C4) (pin 1))
      (node (ref J3) (pin 2))
      (node (ref U2) (pin 13))
      (node (ref J3) (pin 1))
      (node (ref U1) (pin 14))
      (node (ref C1) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref U2) (pin 14)))
    (net (code 6) (name OUT2)
      (node (ref U2) (pin 2))
      (node (ref U2) (pin 5))
      (node (ref J3) (pin 9))
      (node (ref U2) (pin 9))
      (node (ref R9) (pin 1)))
    (net (code 7) (name "Net-(JP2-Pad1)")
      (node (ref R13) (pin 1))
      (node (ref R14) (pin 1))
      (node (ref R12) (pin 1))
      (node (ref R11) (pin 1))
      (node (ref JP2) (pin 1)))
    (net (code 8) (name "Net-(J1-Pad1)")
      (node (ref R6) (pin 1))
      (node (ref J1) (pin 1))
      (node (ref U1) (pin 12))
      (node (ref R7) (pin 2))
      (node (ref JP1) (pin 2)))
    (net (code 9) (name "Net-(J2-Pad1)")
      (node (ref R15) (pin 2))
      (node (ref R14) (pin 2))
      (node (ref J2) (pin 1))
      (node (ref JP2) (pin 2))
      (node (ref U2) (pin 12)))
    (net (code 10) (name "Net-(JP1-Pad1)")
      (node (ref R3) (pin 1))
      (node (ref R4) (pin 1))
      (node (ref JP1) (pin 1))
      (node (ref R6) (pin 2))
      (node (ref R5) (pin 1)))
    (net (code 11) (name "Net-(JP1-Pad3)")
      (node (ref R8) (pin 1))
      (node (ref JP1) (pin 3)))
    (net (code 12) (name "Net-(JP2-Pad3)")
      (node (ref R16) (pin 1))
      (node (ref JP2) (pin 3)))
    (net (code 13) (name "Net-(R5-Pad2)")
      (node (ref U1) (pin 8))
      (node (ref R5) (pin 2)))
    (net (code 14) (name "Net-(R4-Pad2)")
      (node (ref R4) (pin 2))
      (node (ref U1) (pin 6)))
    (net (code 15) (name "Net-(R3-Pad2)")
      (node (ref R3) (pin 2))
      (node (ref U1) (pin 3)))
    (net (code 16) (name IN2)
      (node (ref U2) (pin 11))
      (node (ref J3) (pin 11)))
    (net (code 17) (name OE2)
      (node (ref R10) (pin 1))
      (node (ref U2) (pin 4))
      (node (ref J3) (pin 7))
      (node (ref U2) (pin 10))
      (node (ref U2) (pin 1)))
    (net (code 18) (name "Net-(J3-Pad6)")
      (node (ref J3) (pin 6)))
    (net (code 19) (name "Net-(J3-Pad5)")
      (node (ref J3) (pin 5)))
    (net (code 20) (name IN1)
      (node (ref U1) (pin 11))
      (node (ref J3) (pin 12)))
    (net (code 21) (name OUT1)
      (node (ref U1) (pin 9))
      (node (ref U1) (pin 2))
      (node (ref U1) (pin 5))
      (node (ref J3) (pin 10))
      (node (ref R1) (pin 1)))
    (net (code 22) (name OE1)
      (node (ref U1) (pin 1))
      (node (ref J3) (pin 8))
      (node (ref U1) (pin 4))
      (node (ref U1) (pin 10))
      (node (ref R2) (pin 1)))))